|  |  |  |
| --- | --- | --- |
| Obraz zawierający obiekt, lampa  Opis wygenerowany automatycznie |  |  |

**Cooking sugar rocket grain safety rules**

1. Keep your workspace clean.
2. Have a fire extinguisher nearby.
3. Wear a full protective gear (leather gloves, flame-proof jacket, and complete face shield) while cooking and casting a carmel.
4. Do not inhale a potassium nitrate or vapor, as it may be toxic.
5. Every activity with explosives requires special caution. Nobody shall approach them without respecting following safety rules.
6. Always make sure, that there are no potential heat, fire or spark source near the explosives. Avoid impact, friction, electricity.
7. Use only non-spark producing tools.
8. Any spilled powder shall be secured.
9. Since the two constituents are blended together, the powdered mixture should be handled with due care and kept in a closed container until ready to be cooked.
10. Heating the propellant mixture must only be done using a thermostatically controlled heating vessel.
11. Discard any left-over, unused or unsuitable carmel by dissolving in hot water.